	Front/Back Door Acceleration (100%/s²)

[const]
ffdoor_acc
3

[const]
mfdoor_acc
3

[const]
bfdoor_acc
3

[const]
fadoor_acc
3

[const]
madoor_acc
3

[const]
badoor_acc
3

	Door Acceleration Variation (100%/s²)

[const]
door_acc_var
0.0

[const]
door0_pos_z_speed
15

[const]
door0_pos_z_speed_up
1.5

[const]
door1_pos_z_speed
7

[const]
door1_pos_z_speed_up
3

[const]
door2_pos_z_speed
15

[const]
door2_pos_z_speed_up
2

[const]
door3_pos_z_speed
8

[const]
door3_pos_z_speed_up
2

[const]
door4_pos_z_speed
30

[const]
door4_pos_z_speed_up
2

[const]
door5_pos_z_speed
8

[const]
door5_pos_z_speed_up
2

[newcurve]
door_inc_dblFrontG

[pnt]
0
0

[pnt]
0.5
0.64

[pnt]
0.87
0.94

[pnt]
1
1

[newcurve]
door_inc_dblFrontD

[pnt]
0
0

[pnt]
0.35
0.505

[pnt]
0.7
0.83

[pnt]
1
1

[newcurve]
door_inc_dblRearG

[pnt]
0
0

[pnt]
0.35
0.505

[pnt]
0.7
0.83

[pnt]
1
1

[newcurve]
door_inc_dblRearD

[pnt]
0
0

[pnt]
0.35
0.505

[pnt]
0.7
0.83

[pnt]
1
1

[newcurve]
door_inc_dblAftG

[pnt]
0
0

[pnt]
0.35
0.505

[pnt]
0.7
0.83

[pnt]
1
1

[newcurve]
door_inc_dblAftD

[pnt]
0
0

[pnt]
0.35
0.505

[pnt]
0.7
0.83

[pnt]
1
1
	Front/Back Door Max Speed (100%/s)

[const]
ffdoor_maxspeed
1

[const]
mfdoor_maxspeed
1

[const]
bfdoor_maxspeed
1

[const]
fadoor_maxspeed
1

[const]
madoor_maxspeed
1

[const]
badoor_maxspeed
1

[const]
door_maxspeed_var
0

	Front/Back Door Damper (100%/s)

[const]
door0_damper
0.1

[const]
door1_damper
0.1

[const]
door2_damper
0.1

[const]
door3_damper
0.1

[const]
door4_damper
0.1

[const]
door5_damper
0.1


		Dämpferkennlinie über Öffnungzustand:

[newcurve]
damper_f_close

[pnt]
0
1

[newcurve]
damper_f_open

[pnt]
0
1

[newcurve]
damper_m_close

[pnt]
0
1

[newcurve]
damper_m_open

[pnt]
0
1

[newcurve]
damper_b_close

[pnt]
0
1

[newcurve]
damper_b_open

[pnt]
0
1

	Door Stop Reflexion Coefficient

[const]
door0_refl_opn
0.9

[const]
door1_refl_opn
0.9

[const]
door2_refl_opn
0.9

[const]
door3_refl_opn
0.9

[const]
door4_refl_opn
0.9

[const]
door5_refl_opn
0.9

[const]
door0_refl_cls
0.0

[const]
door1_refl_cls
0.0

[const]
door2_refl_cls
0.0

[const]
door3_refl_cls
0.0

[const]
door4_refl_cls
0.0

[const]
door5_refl_cls
0.0

	Automatic Back Door Time

[const]
doorMidOpenTime
2

[const]
doorAftOpenTime
2

	Busstop Brake will only be activated belov MaxKMH:

[const]
Door_Bremse_Halte_MaxKMH
2

'Vordertürflügel sind kombiniert und Hintertüren manuell:

[const]
door_ManBackDoorFrontDoorCombined
0

'Sicherheits-Rebelüftung:

[const]
door_safe_reactivating
1

[const]
door_stop_request_killed_by_front_door
0

[const]
door_druckluft
0

[const]
door_needs_stopbrake
1

[const]
door_needs_stopbrakeswitch
1

[const]
electric_doors
1

[const]
thinking_doors
0

[const]
door_blocking
0

[const]
door_blocking_area
0.1

[const]
door_blocking_diff
0.03

[const]
door_blocking_speed
0.01

[newcurve]
door_0_opn_speed

[pnt]
0
0.5

[pnt]
0.2
0.5

[pnt]
1
0.2


[newcurve]
door_0_cls_speed

[pnt]
0
0.35

[pnt]
0.35
0.45

[pnt]
0.55
0.1

[pnt]
0.6
0.1

[pnt]
0.7
0.4

[pnt]
0.95
0.33

[pnt]
0.98
0.01

[pnt]
1
0.01

[newcurve]
door_1_opn_speed

[pnt]
0
0.3

[pnt]
0.4
0.4

[pnt]
0.45
0.1

[pnt]
0.5
0.1

[pnt]
0.55
0.5

[pnt]
0.75
0.5

[pnt]
0.80
0.1

[pnt]
0.90
0.1

[pnt]
1
0.5

[newcurve]
door_1_cls_speed

[pnt]
0
0.35

[pnt]
0.35
0.45

[pnt]
0.55
0.1

[pnt]
0.6
0.1

[pnt]
0.7
0.4

[pnt]
0.95
0.3

[pnt]
0.98
0.09

[pnt]
1
0.05


[newcurve]
door_2_opn_speed

[pnt]
0
0.3

[pnt]
0.5
0.4

[pnt]
0.55
0.1

[pnt]
0.75
0.1

[pnt]
0.8
0.4

[pnt]
0.85
0.4

[pnt]
0.9
0.1

[pnt]
1
0.1

[newcurve]
door_2_cls_speed

[pnt]
0
0.3

[pnt]
0.35
0.5

[pnt]
0.55
0.15

[pnt]
0.6
0.15

[pnt]
0.7
0.5

[pnt]
0.95
0.3

[pnt]
0.98
0.05

[pnt]
1
0.05

[newcurve]
door_3_opn_speed

[pnt]
0
0.3

[pnt]
0.4
0.4

[pnt]
0.45
0.1

[pnt]
0.5
0.1

[pnt]
0.55
0.5

[pnt]
0.75
0.5

[pnt]
0.80
0.1

[pnt]
0.90
0.1

[pnt]
1
0.5

[newcurve]
door_3_cls_speed

[pnt]
0
0.3

[pnt]
0.35
0.5

[pnt]
0.55
0.15

[pnt]
0.6
0.15

[pnt]
0.7
0.5

[pnt]
0.95
0.3

[pnt]
0.98
0.05

[pnt]
1
0.05

[newcurve]
door_4_opn_speed

[pnt]
0
0.5

[pnt]
0.2
0.6

[pnt]
0.8
0.6

[pnt]
1
0.5

[newcurve]
door_4_cls_speed

[pnt]
0
0.2

[pnt]
0.17
0.2

[pnt]
0.2
0.7

[pnt]
0.9
0.7

[pnt]
0.97
0.1

[pnt]
0.99
0

[pnt]
1
0.9

[newcurve]
door_5_opn_speed

[pnt]
0
0.3

[pnt]
0.4
0.4

[pnt]
0.45
0.1

[pnt]
0.5
0.1

[pnt]
0.55
0.5

[pnt]
0.75
0.5

[pnt]
0.80
0.1

[pnt]
0.90
0.1

[pnt]
1
0.5

[newcurve]
door_5_cls_speed

[pnt]
0
0.3

[pnt]
0.35
0.5

[pnt]
0.55
0.15

[pnt]
0.6
0.15

[pnt]
0.7
0.5

[pnt]
0.95
0.3

[pnt]
0.98
0.05

[pnt]
1
0.05

[newcurve]
door2_xposition

[pnt]
0
0

[pnt]
0
0


[pnt]
0.1
0.86

[pnt]
0.2
0.86

[pnt]
0.3
0.86

[pnt]
0.4
0.86

[pnt]
0.5
0.86

[pnt]
0.6
0.86

[pnt]
0.7
0.86

[pnt]
0.8
0.86

[pnt]
0.9
0.86

[pnt]
1
0.86


[newcurve]
door2_yposition

[pnt]
0
0

[pnt]
1
1

[newcurve]
door3_xposition

[pnt]
0
0

[pnt]
0
0


[pnt]
0.1
0.86

[pnt]
0.2
0.86

[pnt]
0.3
0.86

[pnt]
0.4
0.86

[pnt]
0.5
0.86

[pnt]
0.6
0.86

[pnt]
0.7
0.86

[pnt]
0.8
0.86

[pnt]
0.9
0.86

[pnt]
1
0.86


[newcurve]
door3_yposition

[pnt]
0
0

[pnt]
1
1


=============================================
Inverse Widerstände (Leitwerte) in 1/Ohm.


Türflügelstromverbrauch: 500W/Geschwindigkeit 1 (0.87 1/Ohm)

[const]
door_Rinv
0.87

.............................