
[const]
engine_J
3.5

[const]
Exhaust_brake_enabled
1

[newcurve]
Exhaust_brake

[pnt]
650
-50

[pnt]
2500
-350


[const]
engine_consumption_curve_available
1

[const]
engine_e-gas
1

[const]
engine_ASR
1

1=default
2=automotive throttle 50 percent equals 50 percent engine torque 
[const]
throttle_type
2

[const]
engine_RPM_ign_cold
150

[const]
engine_RPM_ign_warm
100

	Zeit [s], wie lange er "orgelt", wenn er gerade so die untere, "warme" Grenzdrehzahl erreicht:

[const]
engine_RPM_ign_time2warm
4

[const]
engine_startering_sound_n_max
450

--------------------------------------------------------------------------
Turbocharger controls
--------------------------------------------------------------------------


2 enables the puff limiter/smoke contol most diesels has this enabled. 
[const]
turbochaged
1

[const]
smoke_limiter
0.6

Standard Turbochargers spools way slower then the VGT turbochargers
[const]
VGT_turbochager
0


--------------------------------------------------------------------------
Turbocharger Dynamics
--------------------------------------------------------------------------


Number of liters the engine has (CID) 
this helps calculate the spool rate
of the turbocharger

[const]
engine_CID
4.0

[const]
engine_volumetric_efficiency
96

Value in mm
[const]
turbo_compressor_wheel_size
70


[const]
turbo_min_psi
-1


[const]
turbo_max_psi
45.4045285
    24.4045285


Pressure Ratio starts at 1:1, so an second  value at 0 would yield a pressure ratio of 1:1 or 14.7 PSI Non Aspirate Pressure with 0 PSI turbocharge boost.

Mutipler

[newcurve]
turbo_boost_threshold


[pnt]
500
0.59322033898

[pnt]
1000
1



[newcurve]
turbo_exhaust_flow

[pnt]
50
-1

[pnt]
150
16.29

[pnt]
200
26.29

[pnt]
300
44.11

[pnt]
400
50.46

[pnt]
600
60.1

--------------------------------------------------------------------------
RPM and Speed Governor controls
--------------------------------------------------------------------------

[const]
rpmgov_unload
2900

[const]
rpmgov
2970

[const]
engine_governed_idle_RPM
600

[newcurve]
idle_ctr

[pnt]
-50
1


[pnt]
50
0

[newcurve]
rpmgov_map

[pnt]
-50
1

[pnt]
0
0

    Limitador de velocidade: coloque 0 para desativar
[const]
engine_speedcontrol
1

    Limite de velocidade do limitador (em km/h)
[const]
speedgov
80

--
throttle control
--
[newcurve]
engine_throttle_sensitivity

[pnt]
0
0


[pnt]
1
1

------------------------
Speed Governor thershold 
------------------------

[newcurve]
governor


[pnt]
0
1

[pnt]
1
0

[pnt]
1.01
0

--------------------------------------------------------------------------
Performance Data units in NM
--------------------------------------------------------------------------

[newcurve]
engine_M_maxThrottle


[pnt]
300
145

[pnt]
300
150

[pnt]
550
155

[pnt]
600
167

[pnt]
800
176

[pnt]
1000
196

[pnt]
1100
206

[pnt]
1200
245

[pnt]
1300
275

[pnt]
1600
294

[pnt]
1800
294

[pnt]
2000
265

[pnt]
2200
255

[pnt]
2400
255


[pnt]
2600
0

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
150
300

[pnt]
300
250

[pnt]
592
0

[pnt]
650
-15

[pnt]
1000
-110

[pnt]
2500
-125

[const]
engine_coldM
-300 


--------------------------------------------------------------------------
Fuel Performance Data
--------------------------------------------------------------------------


[newcurve]
engine_consumption_per_rpm

[pnt]
0
0

[pnt]
0
120


[pnt]
800
195


[pnt]
1100
190


[pnt]
1900
211


[pnt]
2800
255

[pnt]
4800
415


[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
0.6

[pnt]
1200
0.7

[pnt]
1700
0.5

[pnt]
2300
0.2

[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1.2



[const]
engine_fuel_value
11.8
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
90


--------------------------------------------------------------------------
Engine Cooling Data
--------------------------------------------------------------------------

[const]
luefterthermostat_opn
91

[const]
luefterthermostat_cls
87


    Thermostat Open Temperature 
[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
82




[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
600

[const]
engine_Qrate_fan_factor
1.3

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
2.8

[const]
engine_cvm_engine
1180000

[const]
engine_cvm_envir
10000

















[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100



[newcurve]
torquelimit

[pnt]
90
1850

[pnt]
105
850

[pnt]
130
300
