
	[friendlyname]
Urbino IV Pack by Iwo k++ - TouchDash
FL|SU18|Electric|ZF AVE|4Dn
Wybierz malowanie

[sound]
Sound_IV\FL_U18_B_Electric_TSA_TMF_BW.cfg

[sound_ai]
Sound_IV\FL_U18_B_Electric_TSA_TMF_BW.cfg

[model]
model\ADIC_FL_Urbino_18_Electric_New_TouchDash_PL_4D_TSA_TMF_B.cfg

[scriptshare]

[paths]
model\paths_SU18_B.cfg

[passengercabin]
model\passengercabin_SU18_B_EV_TSA_new.cfg

	////////////////////////////////////////////////////////
		Scripts
	////////////////////////////////////////////////////////

[varnamelist]
25
Script_IV\AI_varlist.txt
Script_IV\Collision_varlist.txt
Script_IV\antrieb_varlist.txt
Script_IV\engine_varlist.txt
Script_IV\elec_varlist.txt
Script_IV\bremse_varlist.txt
Script_IV\auspuff_varlist.txt
Script_IV\lights_varlist.txt
Script_IV\door_varlist.txt
Script_IV\wiper_varlist.txt
Script_IV\cockpit_varlist.txt
Script_IV\klappern_varlist.txt
Script_IV\heizung_varlist.txt
Script_IV\rain_varlist.txt
Script_IV\dirt_varlist.txt
Script_IV\ticketprinter_varlist.txt
Script_IV\wimpel_varlist.txt
Script_IV\visual_varlist.txt
Script_IV\cashdesk_varlist.txt
Script_IV\VDV_varlist.txt
Script_IV\spray_varlist.txt
Script_IV\TACTILEO\IBIS_varlist.txt
Script_IV\TACTILEO\ineo_varlist.txt
Script_IV\churaKrueger\VMatrix_varlist.txt
Script_IV\articulation_varlist.txt

[stringvarnamelist]
6
Script_IV\ticketprinter_stringvarlist.txt
Script_IV\TACTILEO\IBIS_stringvarlist.txt
Script_IV\TACTILEO\ineo_stringvarlist.txt
Script_IV\cockpit_stringvarlist.txt
Script_IV\VDV_stringvarlist.txt
Script_IV\churaKrueger\VMatrix_stringvarlist.txt


	////////////////////////////////////////////////////////
		Kameras *NEU01*
	////////////////////////////////////////////////////////


	0: Blick nach vorne (std)
[add_camera_driver]
0
4.68
1.84
-0.06
45
0
-10



################
Passagiersichten
################

	0: Hinten links sitzend
[add_camera_pax]
-0.953875
0.216584
2
-0.06
50
15
0

	1: Stehplatz an der Hintertuer
[add_camera_pax]
-0.95
1.39315
2.05
-0.06
60
90
-12
	2: vorne rechts sitzend
[add_camera_pax]
0.88
-0.688521
2
-0.06
45
-20
0

	4: hinten rechts sitzend
[add_camera_pax]
0.121953
-3.40425
2.1
-0.06
45
0
0

	5: hinten rechts sitzend
[add_camera_pax]
0
4.5
2.1
-0.06
60
180
-10

	4: hinten rechts sitzend
[add_camera_pax]
0
-1.8
2.0
-0.06
45
0
0

	6: Na zewnatrz z zoomem
[add_camera_pax]
12
30
1.4
-0.06
38
0
-10

	7: Na zewnatrz z zoomem
[add_camera_pax]
-12
30
1.4
-0.06
38
0
-10

	6: Na zewnatrz z zoomem
[add_camera_pax]
12
30
1.4
-0.06
38
0
-10

	7: Na zewnatrz z zoomem
[add_camera_pax]
-12
30
1.4
-0.06
38
0
-10

	10: kek1
[add_camera_pax]
-3.0
-1.8
2.0
20.0
60
0
0

	11: Tele-Lens
[add_camera_pax]
0.0
-1.8
2.0
40.0
45
0
0

	12: kek
[add_camera_pax]
3.0
-1.8
2.0
20.0
60
0
0

	13: kek
[add_camera_pax]
0
-0.5
1.65034
15
100
64
0

	14: by vavilon4eg59
[add_camera_pax]
5.5
20.0
1.7
0.05
64
-140
0
	15: by vavilon4eg59
[add_camera_pax]
-5.5
20.0
1.7
0.05
64
140
0
	13: by vavilon4eg59
[add_camera_pax]
5.5
-20.0
1.7
0.05
64
-40
0

	Folgender Befehl setzt die Standardfahrerkamera:

[set_camera_std]
3

	Folgender Befehl setzt den Zentrierpunkt der AuЯenkamera:

[set_camera_outside_center]
0
0
1.2



////////////////////////////////////////////////////////
Physikalische und geometrische Grunddaten
////////////////////////////////////////////////////////

[mass]
7

500
250
500

[momentofintertia]
150
40
180

[boundingbox]
2.52
7.5
2.4
0
-0.1
1.8

[cog]
0
0
00.3

[schwerpunkt]
1.2

[rollwiderstand]
500

[rot_pnt_long]
-0.28711

[ai_deltaheight]
-0.10


Hinterachse:

[newachse]
achse_long
-0.28711
achse_maxwidth
2.42
achse_minwidth
1.2
achse_raddurchmesser
0.94
achse_feder
320
achse_maxforce
115
achse_daempfer
17
achse_antrieb
1

[coupling_front]
0
3.8689
0.53

[couple_front_open_for_sound]

[coupling_front_character]
52.5
-20
20
1