	WEG 250kW 615v

[const]
engine_J
3.0

[const]
engine_speedcontrol
0

[const]
engine_e-gas
1

[const]
engine_ASR
1

[const]
engine_governed_idle_RPM
600

[const]
engine_governed_max_RPM
2200

[const]
engine_power_idle
22000

[const]
engine_coldM
-350

[newcurve]
engine_M_maxThrottle

[pnt]
300
2800

[pnt]
500
2800

[pnt]
700
2800

[pnt]
900
2800

[pnt]
1200
2800

[pnt]
1670
2800

[pnt]
1800
2800

[pnt]
2000
2800

[pnt]
2100
2800

[pnt]
3200
2800

[pnt]
3450
2800

[pnt]
3700
0

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
300
250

[pnt]
592
0

[pnt]
650
-1

[pnt]
1000
-30

[pnt]
2500
-35

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
250
0.25

[pnt]
375
0.5

[pnt]
500
0.75

[pnt]
1000
1

[pnt]
1500
0.75

[pnt]
2000
0.5

[pnt]
2500
0.25

[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1.2

[const]
engine_fuel_value
12.2
10.00
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
131


[const]
luefterthermostat_opn
90

[const]
luefterthermostat_cls
90

[const]
kuehlerthermostat_opn
90

[const]
kuehlerthermostat_cls
90

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
300

[const]
engine_Qrate_fan_factor
1.15

[const]
engine_Qrate_veloc_factor_basic
300

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
550000

[const]
engine_cvm_envir
10000



