[const]
engine_J
3.5

[const]
engine_speedcontrol
0

[const]
engine_e-gas
1

[const]
engine_ASR
1

[const]
engine_governed_idle_RPM
592

[const]
engine_power_idle
22710

[const]
engine_coldM
-300

[newcurve]
engine_n_coldM

[pnt]
0
-140

[pnt]
2500
-350


[const]
engine_oelvis_M_nulldeg
-20

[const]
engine_oelvis_M_expfactor
-0.05

[const]
engine_RPM_ign_cold
150

[const]
engine_RPM_ign_warm
100

	Zeit [s], wie lange er "orgelt", wenn er gerade so die untere, "warme" Grenzdrehzahl erreicht:

[const]
engine_RPM_ign_time2warm
4


[const]
engine_starterM
1000

[const]
engine_starter_n_halbwert
67

[const]
engine_startering_sound_n_max
450

Mindeststrom, der immer durch den Starter fließt

[const]
engine_starter_minI
300

Ampere/Nm:

[const]
engine_starter_Ifaktor
0.5

[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
150
700

[pnt]
300
800

[pnt]
592
900

[pnt]
600
850

[pnt]
1000
800

[pnt]
1400
760

[pnt]
1900
750

[pnt]
2100
741

[pnt]
2300
730

[pnt]
2350
0

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
150
30

[pnt]
300
30

[pnt]
592
-100

[pnt]
650
-200

[pnt]
1000
-300

[pnt]
2500
-350

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
0.8

[pnt]
1200
0.65

[pnt]
1700
0.65

[pnt]
2300
0.3

[newcurve]
engine_efficiency_throttle

[pnt]
0
1.9

[pnt]
0.8
1.5

[pnt]
1
1.5

[const]
engine_fuel_value
16
9.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250



[const]
luefterthermostat_opn
90

[const]
luefterthermostat_cls
87

[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
82

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
300

[const]
engine_Qrate_fan_factor
1.15

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000