	Front/Back Door Acceleration (100%/s²)

[const]
fdoor_acc
1.5

[const]
mdoor_acc
1.5

[const]
bdoor_acc
1.5

===========

[const]
fdoor_acc_elec
0.55

[const]
mdoor_acc_elec
0.57

[const]
bdoor_acc_elec
0.54

===========

[const]
fdoor_acc_swing_e4
0.54

[const]
mdoor_acc_swing_e4
0.5

[const]
bdoor_acc_swing_e4
0.48

===========

[const]
fdoor_acc_sliding
3

[const]
mdoor_acc_sliding
2.9

[const]
bdoor_acc_sliding
2.8

	Door Acceleration Variation (100%/s²)

[const]
door_acc_var
0.02

	Door gap time (s)

[const]
door01_open_gap
0.25

[const]
door01_close_gap
0.25

[const]
door23_open_gap
0.25

[const]
door23_close_gap
0.25

[const]
door45_open_gap
0.25

[const]
door45_close_gap
0.25

[const]
door67_open_gap
0.25

[const]
door67_close_gap
0.25

	Front/Back Door Max Speed (100%/s)

[const]
fdoor_maxspeed
1.0

[const]
mdoor_maxspeed
0.95

[const]
bdoor_maxspeed
0.92

===========

[const]
fdoor_maxspeed_elec
0.4

[const]
mdoor_maxspeed_elec
0.42

[const]
bdoor_maxspeed_elec
0.47

===========

[const]
fdoor_maxspeed_swing_e4
0.55

[const]
mdoor_maxspeed_swing_e4
0.52

[const]
bdoor_maxspeed_swing_e4
0.5

===========

[const]
fdoor_maxspeed_sliding
0.1

[const]
mdoor_maxspeed_sliding
0.1

[const]
bdoor_maxspeed_sliding
0.1

[const]
door_maxspeed_var
0.02

	Front/Back Door Damper (100%/s)

[const]
door0_damper
3

[const]
door1_damper
3

[const]
door2_damper
3

[const]
door3_damper
2

[const]
door4_damper
3

[const]
door5_damper
2

[const]
door6_damper
3

[const]
door7_damper
2


		Dämpferkennlinie über Öffnungzustand:

[newcurve]
damper_f_close

[pnt]
0.2
0.8

[pnt]
0.8
0.1

[newcurve]
damper_f_open

[pnt]
0.2
0.1

[pnt]
0.8
0.8

[newcurve]
damper_m_close

[pnt]
0.2
1

[pnt]
0.8
0.1

[newcurve]
damper_m_open

[pnt]
0.2
0.1

[pnt]
0.8
0.6

[newcurve]
damper_b_close

[pnt]
0.2
1

[pnt]
0.8
0.1

[newcurve]
damper_b_open

[pnt]
0.2
0.1

[pnt]
0.8
0.6

	Door Stop Reflexion Coefficient

[const]
door_refl
0.01

	Busstop Brake will only be activated belov MaxKMH:

[const]
Door_Bremse_Halte_MaxKMH
4

'Vordertürflügel sind kombiniert und Hintertüren manuell:

[const]
door_ManBackDoorFrontDoorCombined
1

'Sicherheits-Rebelüftung:

[const]
door_safe_reactivating
0

[const]
door_stop_request_killed_by_front_door
0

[const]
door_druckluft
1

[const]
door_needs_stopbrake
1

[const]
door_needs_stopbrakeswitch
1

[const]
thinking_doors
0

[const]
door_blocking
1

[const]
door_blocking_area
0.1

[const]
door_blocking_diff
0.03

[const]
door_blocking_speed
0.1

[newcurve]
door_0_opn_speed

[pnt]
0
1

[newcurve]
door_0_cls_speed

[pnt]
0
1

[newcurve]
door_1_opn_speed

[pnt]
0
1

[newcurve]
door_1_cls_speed

[pnt]
0
1

[newcurve]
door_2_opn_speed

[pnt]
0
1

[newcurve]
door_2_cls_speed

[pnt]
0
1

[newcurve]
door_3_opn_speed

[pnt]
0
1

[newcurve]
door_3_cls_speed

[pnt]
0
1

[newcurve]
door_4_opn_speed

[pnt]
0
1

[newcurve]
door_4_cls_speed

[pnt]
0
1

[newcurve]
door_5_opn_speed

[pnt]
0
1

[newcurve]
door_5_cls_speed

[pnt]
0
1

[newcurve]
door_6_opn_speed

[pnt]
0
1

[newcurve]
door_6_cls_speed

[pnt]
0
1

[newcurve]
door_7_opn_speed

[pnt]
0
1

[newcurve]
door_7_cls_speed

[pnt]
0
1


[newcurve]
door_0_opn_speed_sliding

[pnt]
0
0.1

[pnt]
0.2
0.5


[pnt]
0.8
0.6

[pnt]
1
0.1

[newcurve]
door_0_cls_speed_sliding

[pnt]
0
0.1

[pnt]
0.2
0.7

[pnt]
0.8
0.8

[pnt]
1
0.1

[newcurve]
door_1_opn_speed_sliding

[pnt]
0
0.1

[pnt]
0.2
0.5


[pnt]
0.8
0.6

[pnt]
1
0.1

[newcurve]
door_1_cls_speed_sliding

[pnt]
0
0.1

[pnt]
0.2
0.7

[pnt]
0.8
0.8

[pnt]
1
0.1

[newcurve]
door_1_opn_speed_sliding_U

[pnt]
0
0.1

[pnt]
0.2
0.5


[pnt]
0.8
0.6

[pnt]
1
0.1

[newcurve]
door_1_cls_speed_sliding_U

[pnt]
0
0.1

[pnt]
0.2
0.7

[pnt]
0.8
0.8

[pnt]
1
0.1

[newcurve]
door_2_opn_speed_sliding

[pnt]
0
0.1

[pnt]
0.2
0.6


[pnt]
0.8
0.7

[pnt]
1
0.1

[newcurve]
door_2_cls_speed_sliding

[pnt]
0
0.1

[pnt]
0.2
0.7

[pnt]
0.8
0.7

[pnt]
1
0.1

[newcurve]
door_3_opn_speed_sliding

[pnt]
0
0.1

[pnt]
0.2
0.6


[pnt]
0.8
0.7

[pnt]
1
0.1

[newcurve]
door_3_cls_speed_sliding

[pnt]
0
0.1

[pnt]
0.2
0.7

[pnt]
0.8
0.7

[pnt]
1
0.1

[newcurve]
door_4_opn_speed_sliding

[pnt]
0
0.1

[pnt]
0.2
0.6


[pnt]
0.8
0.7

[pnt]
1
0.1

[newcurve]
door_4_cls_speed_sliding

[pnt]
0
0.1

[pnt]
0.2
0.7

[pnt]
0.8
0.7

[pnt]
1
0.1

[newcurve]
door_5_opn_speed_sliding

[pnt]
0
0.1

[pnt]
0.2
0.6


[pnt]
0.8
0.7

[pnt]
1
0.1

[newcurve]
door_5_cls_speed_sliding

[pnt]
0
0.1

[pnt]
0.2
0.7

[pnt]
0.8
0.7

[pnt]
1
0.1

[newcurve]
door_5_opn_speed_sliding_U

[pnt]
0
0.1

[pnt]
0.2
0.6


[pnt]
0.8
0.7

[pnt]
1
0.1

[newcurve]
door_5_cls_speed_sliding_U

[pnt]
0
0.1

[pnt]
0.2
0.7

[pnt]
0.8
0.7

[pnt]
1
0.1

[newcurve]
door_6_opn_speed_sliding

[pnt]
0
0.1

[pnt]
0.2
0.6


[pnt]
0.8
0.7

[pnt]
1
0.1

[newcurve]
door_6_cls_speed_sliding

[pnt]
0
0.1

[pnt]
0.2
0.7

[pnt]
0.8
0.7

[pnt]
1
0.1

[newcurve]
door_7_opn_speed_sliding

[pnt]
0
0.1

[pnt]
0.2
0.6


[pnt]
0.8
0.7

[pnt]
1
0.1

[newcurve]
door_7_cls_speed_sliding

[pnt]
0
0.1

[pnt]
0.2
0.7

[pnt]
0.8
0.7

[pnt]
1
0.1

=============================================
Inverse Widerstände (Leitwerte) in 1/Ohm.


Türflügelstromverbrauch: 150W/Geschwindigkeit 1 (0.260 1/Ohm)

[const]
door_Rinv
0.150

.............................

=============================================
Malfunction-Parameter

[const]
door_malf_autobdoor_livetime_cyc
1000



[newcurve]
door_sliding

[pnt]
0.0
0.0

[pnt]
0.1
1.0

[pnt]
1.0
1.0