Installation

OMSI 1

1. Copy the contents of the package to:
   OMSI\Vehicles\(BUS NAME)\Sound folder.

2. Check which Sound.cfg file is used by the bus.
   Open the .bus file in the bus folder
   Look under the [sound] section to find the correct file.

3. Open the bus’s Sound.cfg file.

4. Delete all sound blocks related to the engine and rear axle.

5. Open the Sound_OMSI.cfg file.

6. Copy its contents into the Sound.cfg file, ensuring that all other sounds remain unchanged.

7. Look in the .BUS-file which engine script the vehicle uses,
   then open it. Search for the word '' Throttle '' and search until you reach the area shown in the script.modofy.bmp-   file. Modify the values ​​based on the image. This only affects
   two numbers. You can find the Image in the Installation folder.
   The upper value should be 10, the lower value should be 8. Although you can change it as you like.

   These two values ​​simulate the time when the Accelerator Pedal is pressed and when it is released.
   By modifying these values, the real accelerator pedal sensitivity of the vehicle can be better simulated.

OMSI 2 Standard Buses

1. Copy the contents of the package to:
   OMSI 2\Vehicles\(BUS NAME)\Sound folder.

2. Check which Sound.cfg file is used by the bus.
   Open the .bus file in the bus folder
   Look under the [sound] section to find the correct file.

3. Open the bus’s Sound.cfg file.

4. Delete all sound blocks related to the engine and rear axle.

5. Open the Sound_OMSI_2.cfg file.

6. Copy its contents into the Sound.cfg file, ensuring that all other sounds remain unchanged.

7. Look in the .BUS-file which engine script the vehicle uses,
   then open it. Search for the word '' Throttle '' and search until you reach the area shown in the script.modofy.bmp-   file. Modify the values ​​based on the image. This only affects
   two numbers. You can find the Image in the Installation folder.
   The upper value should be 10, the lower value should be 8. Although you can change it as you like.

   These two values ​​simulate the time when the Accelerator Pedal is pressed and when it is released.
   By modifying these values, the real accelerator pedal sensitivity of the vehicle can be better simulated.

OMSI 2 Citybus i260/i280 Series

1. Copy the contents of the package to:
   OMSI 2\Vehicles\(CITYBUS 260/280 NAME)\Sound folder.

2. Check which Sound.cfg file is used by the bus.
   Open the .bus file in the bus folder.
   Look under the [sound] section to find the correct file.

3. Open the bus’s Sound.cfg file.

4. Delete all sound blocks related to the engine and rear axle,
   
   EXCEPT!

   Do NOT delete the original engine start and stop sound blocks.
   Removing these lines will prevent the bus from functioning in the game.

5. Open the Sound_CITYBUS.cfg file.

6. Copy its contents into the Sound.cfg file, ensuring that all other sounds remain unchanged.

7. Look in the .BUS-file which engine script the vehicle uses,
   then open it. Search for the word '' Throttle '' and search until you reach the area shown in the script.modofy.bmp-   file. Modify the values ​​based on the image. This only affects
   two numbers. You can find the Image in the Installation folder.
   The upper value should be 10, the lower value should be 8. Although you can change it as you like.

   These two values ​​simulate the time when the Accelerator Pedal is pressed and when it is released.
   By modifying these values, the real accelerator pedal sensitivity of the vehicle can be better simulated.