[const]
engine_J
3.5

[const]
engine_speedcontrol
0

[const]
engine_e-gas
1

[const]
engine_ASR
0

[const]
engine_governed_idle_RPM
592

[const]
engine_power_idle
27000

[const]
engine_coldM
-300

[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
300
300

[pnt]
500
500

[pnt]
1000
600

[pnt]
1500
700

[pnt]
2000
750

[pnt]
2500
800

[pnt]
3000
850

[pnt]
3500
860

[pnt]
4000
870

[pnt]
4500
880

[pnt]
5000
890

[pnt]
5500
900

[pnt]
6000
890

[pnt]
6500
870

[pnt]
7000
840

[pnt]
7500
750

[pnt]
8000
700

[pnt]
8500
500

[pnt]
9000
0

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
300
250

[pnt]
592
0

[pnt]
650
-200

[pnt]
1000
-400

[pnt]
2500
-450

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
1

[pnt]
1200
1

[pnt]
1700
1

[pnt]
2300
1

[pnt]
3000
1.2

[pnt]
3500
1.5

[pnt]
4000
1.7 

[pnt]
4500
2

[pnt]
5000
2.1

[pnt]
5500
2.2

[pnt]
6000
2.3

[pnt]
6500
2.4

[pnt]
7000
2.6

[pnt]
7500
2.4

[pnt]
8000
2

[pnt]
8500
1.3

[pnt]
9000
0

[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1.5

[pnt]
1
2

[const]
engine_fuel_value
16
9.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250


[const]
luefterthermostat_opn
90

[const]
luefterthermostat_cls
87

[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
82

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
300

[const]
engine_Qrate_fan_factor
1.15

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000

