[const]
engine_J
3.5

[const]
engine_brake
1

[const]
engine_consumption_curve_available
1

[const]
engine_speedcontrol
0

[const]
smoke_limiter
0.7

[const]
engine_e-gas
1

[const]
engine_ASR
1

[const]
speedgov
100


[const]
rpmgov_unload
2300

[const]
rpmgov
2300

[const]
turbochaged
1


[const]
engine_governed_idle_RPM
650

Amount of watts used up during idle

[const]
engine_power_idle
25124

[const]
engine_coldM
-300 

[const]
engine_braking_coeffient
0.74


[newcurve]
fanrpm


[pnt]
600
800


[pnt]
1000
1300

[pnt]
1600
2000



[newcurve]
fanrpm_temp


[pnt]
80
750


[pnt]
86
750


[pnt]
89
1250

[pnt]
92
2000


[newcurve]
fan_kw


[pnt]
600
800


[pnt]
2000
35


[newcurve]
engine_consumption_per_rpm

[pnt]
0
0


[pnt]
800
195


[pnt]
1000
190

[pnt]
1200
195

[pnt]
1400
195

[pnt]
1600
199

[pnt]
1800
206

[pnt]
1900
216

[newcurve]
engine_M_maxThrottle

[pnt]
300
1000

[pnt]
600
1175

[pnt]
700
1310

[pnt]
800
1425

[pnt]
900
1620

[pnt]
1000
1845

[pnt]
1100
1850

[pnt]
1200
1850

[pnt]
1300
1850

[pnt]
1400
1850

[pnt]
1500
1805

[pnt]
1600
1660

[pnt]
1700
1555

[pnt]
1800
1483

[pnt]
1900
1275

[pnt]
2000
1157.09

[pnt]
2100
1051.13







[newcurve]
engine_M_minThrottle

[pnt]
500
-211

[pnt]
700
-311

[pnt]
1000
-391.63


[pnt]
1300
-547.73

[pnt]
1700
-728.24


[pnt]
2300
-728.24

[pnt]
3000
-741.72


Not used just yet
[newcurve]
engine_M_brake

[pnt]
0
0

[pnt]
1200
-1661.46


[pnt]
1500
-1661.46


[pnt]
2200
-1618.30


[newcurve]
engine_efficiency_rpm

[pnt]
0
1

[pnt]
600
1






[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1.2


[newcurve]
engine_braking

[pnt]
0
1

[pnt]
1
0

[const]
engine_fuel_value
11.8
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
460



[const]
luefterthermostat_opn
81

[const]
luefterthermostat_cls
76

[const]
kuehlerthermostat_opn
76

[const]
kuehlerthermostat_cls
72

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
300

[const]
engine_Qrate_fan_factor
2.3

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
800000

[const]
engine_cvm_envir
10000







[newcurve]
governor


[pnt]
0
1

[pnt]
1
0

[pnt]
1.01
0

[newcurve]
rpmgov_map
[pnt]
-100
1

[pnt]
150
0






Pressure Ratio starts at 1:1, so an second  value at 0 would yield a pressure ratio of 1:1 or 14.7 PSI Non Aspirate Pressure with 0 PSI turbocharge boost.

[newcurve]
turbo_exhaust_flow

[pnt]
50
0

[pnt]
144.2
4.35


[pnt]
720
51.45







[const]
engine_volumetric_efficiency
90

Value in mm
[const]
turbo_compressor_wheel_size
86.4


[const]
turbo_min_psi
-1


[const]
turbo_max_psi
21




number of liters the engine has (CID) this helps calculate the spool rate of the turbocharger

[const]
engine_CID
12.1




[newcurve]
idle_ctr

[pnt]
-50
1


[pnt]
50
0




[newcurve]
engine_alternator_load

[pnt]
0
0

[pnt]
850
8.5

[pnt]
3000
11.114




[newcurve]
engine_throttle_sensitivity

[pnt]
0
0

[pnt]
1
1


[newcurve]
engine_throttle_brake

[pnt]
0
1

[pnt]
0.1
0


[const]
VGT_turbochager
0

[newcurve]
engine_temp_glowplug

[pnt]
-10
15

[pnt]
80
2



