'######################
' HAMBURGER STADTBUS SOLO 2012
'######################

[const]
engine_stopdelay
0.6

[const]
dpf_km_intervall
1500

[const]
dpf_rpm_effect
150

[newcurve]
throttle_hyst

[pnt]
0
0

[pnt]
0.15
0.2

[pnt]
0.4
0.6

[pnt]
0.6
0.8

[pnt]
0.85
0.85

[const]
engine_rpm_shake
0.5

[const]
engine_rpm_shake_timer
0.4

[newcurve]
engine_rpm_shake_temp

[pnt]
-30
5

[pnt]
0
2

[pnt]
30
0

[newcurve]
engine_pitch

[pnt]
0
0

[pnt]
549
0.549

[pnt]
1420
1.0

[pnt]
2400
1.7

[newcurve]
engine_bass_sound

[pnt]
0
1

[pnt]
550
1

[pnt]
2400
2

[newcurve]
engine_sound_howl_1

[pnt]
-17
-1

[pnt]
0
0

[pnt]
0.25
0

[pnt]
17
1

[newcurve]
engine_sound_howl_2

[pnt]
0
1

[pnt]
50
2.2

[newcurve]
engine_turbo_RPM_factor

[pnt]
0
0

[pnt]
500
0.5

[pnt]
1200
0.7

[pnt]
1600
0.9

[pnt]
2000
1

[newcurve]
engine_turbo_throttle_factor

[pnt]
0
0.5

[pnt]
1
1

[newcurve]
engine_turbo_boost

[pnt]
0
1

[pnt]
70
1

[pnt]
90
1.3

[pnt]
100
1.4

[newcurve]
speed_reduce

[pnt]
-5
1

[pnt]
0
1

[pnt]
15
1

[const]
engine_sound_gluckern_start
5

[const]
engine_sound_gluckern_stop
186

[const]
euro6_klacken
1

[const]
engine_J
6.0

[const]
engine_speedcontrol
1

[const]
engine_e-gas
1

[const]
engine_ASR
1

[const]
engine_governed_idle_RPM
700

[const]
engine_power_idle
22710

[const]
engine_coldM
-300

[newcurve]
egb_vmax

[pnt]
90.0
1

[pnt]
90.5
0

[newcurve]
engine_startspeed

[pnt]
-100
30

[pnt]
-20
10

[pnt]
0
5

[pnt]
10
0

[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
600
800

[pnt]
1100
1200

[pnt]
1500
1450

[pnt]
2000
900

[pnt]
2050
750

[pnt]
2200
0

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
450
800

[pnt]
585
0

[pnt]
900
-280

[pnt]
1400
-350

[pnt]
2165
-450

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
620
0.85

[pnt]
1300
0.75

[pnt]
1800
0.6

[pnt]
2200
0.4

[pnt]
2350
0.3

[pnt]
2565
0.2

[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1.2

[const]
engine_fuel_value
16
9.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
300


[const]
luefterthermostat_opn
90

[const]
luefterthermostat_cls
87

[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
82

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
0.6

[const]
engine_Qrate_cooling_factor
300

[const]
engine_Qrate_fan_factor
1.15

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
900000

[const]
engine_cvm_envir
10000

