[const]
engine_J
3.55

[const]
engine_speedcontrol
0

[const]
engine_e-gas
0

[const]
engine_ASR
0

[const]
engine_governed_idle_RPM
560

[const]
engine_power_idle
22000

[const]
engine_coldM
-365

[newcurve]
engine_n_coldM

[pnt]
0
-140

[pnt]
1100
-340

[pnt]
1600
-372

[pnt]
2500
-280

[const]
engine_oelvis_M_nulldeg
-20

[const]
engine_oelvis_M_expfactor
-0.05

[const]
engine_RPM_ign_cold
165

[const]
engine_RPM_ign_warm
125

[const]
engine_RPM_ign_izzitas
105

	Zeit [s], wie lange er "orgelt", wenn er gerade so die untere, "warme" Grenzdrehzahl erreicht:

[const]
engine_RPM_ign_time2warm
30

[const]
izzitas_ido
20

[const]
izzitas_ido1
17

[const]
izzitas_ido2
14

[const]
izzitas_ido3
13

[const]
izzitas_ido4
9

[const]
izzitas_ido5
6

[const]
izzitas_ido6
3

[const]
izzitas_ido7
1

[const]
engine_starterM
1065

[const]
engine_starter_n_halbwert
67

[const]
engine_startering_sound_n_max
350

Mindeststrom, der immer durch den Starter fließt

[const]
engine_starter_minI
300

Ampere/Nm:

[const]
engine_starter_Ifaktor
0.5

[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
150
315

[pnt]
300
425

[pnt]
592
525

[pnt]
600
600

[pnt]
800
680

[pnt]
1000
700

[pnt]
1600
765

[pnt]
2000
680

[pnt]
2200
670

[pnt]
2280
0

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
150
300

[pnt]
350
450

[pnt]
500
560

[pnt]
683
0

[pnt]
750
-100

[pnt]
1000
-235

[pnt]
1700
-280

[pnt]
2000
-270

[pnt]
2300
-250

[newcurve]
engine_M_brake

[pnt]
50
0

[pnt]
200
-1175

[pnt]
1000
-250

[pnt]
1500
-345

[pnt]
2000
-487

[pnt]
2500
-521

[const]
engine_brake_only_with_hard_gear
0

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
683
0.6

[pnt]
1200
0.45

[pnt]
1700
0.45

[pnt]
2300
0.2

[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1.2

[const]
engine_fuel_value
16
9.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
240

[const]
luefterthermostat_opn
82

[const]
luefterthermostat_cls
77

[const]
kuehlerthermostat_opn
70

[const]
kuehlerthermostat_cls
65

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100

[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
470

[const]
engine_Qrate_fan_factor
1.6

[const]
engine_Qrate_veloc_factor_basic
210

[const]
engine_Qrate_veloc_factor
5

[const]
engine_cvm_engine
600000

[const]
engine_cvm_kalyha
4000000

[const]
engine_cvm_kalyha1
8000000

[const]
engine_cvm_envir
10000

Max teljesítmény adott fordulatnál
[newcurve]
engine_teljesitmeny

[pnt]
0
0

[pnt]
400
1

[pnt]
1000
1

[pnt]
1800
1.1

[pnt]
2200
1.1220

[pnt]
2300
1.1
