[const]
engine_J
4.0

[const]
engine_speedcontrol
0

[const]
engine_e-gas
0

[const]
engine_ASR
0

[const]
engine_governed_idle_RPM
560

[const]
engine_power_idle
24500

[const]
engine_coldM
-400

[newcurve]
engine_n_coldM

[pnt]
0
-165

[pnt]
1100
-424

[pnt]
2500
-355

[const]
engine_oelvis_M_nulldeg
-20

[const]
engine_oelvis_M_expfactor
-0.05

[const]
engine_RPM_ign_cold
155

[const]
engine_RPM_ign_warm
120

[const]
engine_RPM_ign_izzitas
102

	Zeit [s], wie lange er "orgelt", wenn er gerade so die untere, "warme" Grenzdrehzahl erreicht:

[const]
engine_RPM_ign_time2warm
20

[const]
izzitas_ido
15

[const]
izzitas_ido1
12

[const]
izzitas_ido2
9

[const]
izzitas_ido3
7

[const]
izzitas_ido4
5

[const]
izzitas_ido5
4

[const]
izzitas_ido6
3

[const]
izzitas_ido7
2

[const]
engine_starterM
1065

[const]
engine_starter_n_halbwert
67

[const]
engine_startering_sound_n_max
330

Mindeststrom, der immer durch den Starter fließt

[const]
engine_starter_minI
300

Ampere/Nm:

[const]
engine_starter_Ifaktor
0.5

[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
300
400

[pnt]
600
880

[pnt]
1100
1140

[pnt]
1350
1050

[pnt]
1500
1000

[pnt]
2100
820

[pnt]
2225
698

[pnt]
2380
0

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
150
300

[pnt]
300
328

[pnt]
450
550

[pnt]
510
0

[pnt]
820
-150

[pnt]
2800
-220

[newcurve]
engine_M_brake

[pnt]
50
0

[pnt]
200
-1175

[pnt]
600
-200

[pnt]
1000
-250

[pnt]
1500
-345

[pnt]
2000
-487

[pnt]
2500
-521

[const]
engine_brake_only_with_hard_gear
0

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
768
1

[pnt]
1200
0.45

[pnt]
1700
0.45

[pnt]
2300
0.2

[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1.2

[const]
engine_fuel_value
16
9.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
240

[const]
luefterthermostat_opn
80

[const]
luefterthermostat_cls
75

[const]
kuehlerthermostat_opn
70

[const]
kuehlerthermostat_cls
65

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100

[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
689

[const]
engine_Qrate_fan_factor
1.8

[const]
engine_Qrate_veloc_factor_basic
220

[const]
engine_Qrate_veloc_factor
5

[const]
engine_cvm_engine
600000

[const]
engine_cvm_kalyha
4000000

[const]
engine_cvm_kalyha1
8000000

[const]
engine_cvm_envir
10000

First is turbocharger PSI
Second is the torque mutipler

[newcurve]
turbo_M_max

[pnt]
0
0.85

[pnt]
9
1.0

[pnt]
30
1.1250

[newcurve]
turbo_limit_thorttle_1

[pnt]
0
5

[pnt]
0.82
23

[pnt]
1
30

[newcurve]
turbo_engine_rpm_min_psi

[pnt]
200
0

[pnt]
390
0

[pnt]
460
4.1

[pnt]
490
4.9

[pnt]
2100
10

[newcurve]
turbo_engine_rpm_max_psi

[pnt]
200
0

[pnt]
500
20

[pnt]
1000
28

[pnt]
1500
30

[pnt]
2100
30

[newcurve]
turbo_inertia

[pnt]
0
4

[pnt]
30
6

[newcurve]
turbo_inertia_dec

[pnt]
0
1

[pnt]
5
1

[pnt]
10
5

[pnt]
30
20

[newcurve]
turbo_M_inertia_throttle

[pnt]
0
1


[pnt]
1
1

[newcurve]
engine_airflow

[pnt]
0
1

[pnt]
20
2