
[type]
2

[model]
model\SprzegTyl.cfg

[number]
Regs_A3_64-66_K.org

[registration_automatic]

[rowdy_factor]
0
0

[fixed]

[scriptshare]

[stringvarnamelist]
1
script\tablice_stringvarlist.txt

[varnamelist]
8
script\N_varlist.txt
script\cockpit_varlist.txt
script\drzwi_varlist.txt
script\tablice_varlist.txt
script\swiatla_varlist.txt
script\Panto_varlist.txt
script\rain_varlist.txt
script\wycieraczki_varlist.txt

	////////////////////////////////////////////////////////
		AI parameters:
	////////////////////////////////////////////////////////

	Controls the AI brake behaviour: th

	[ai_brakeperformance]
	{mean AI brake deceleration, [m/s˛] std: 1.0}
	{variation between rowdy factor 0 and 1, [0...1...] std: 0.2}
	{exploit of possible friction, [0...1], std: 0.3}
	{final brake setting, will be used shortly before and while holding, [0...1], std: 0.2}
	{holding point offset, will be used to correct unprecise braking, [m], std: 0}
	

	[ai_brakeperformance]
	1.3
	0.0
	0.8
	1.0
	-1.0

[coupling_front]
0
-3.905
0.41


[coupling_back]
0
-5.746
0.41



	////////////////////////////////////////////////////////
		Drehgestelle (Achsen)
	////////////////////////////////////////////////////////

	Falls Schienenfahrzeug, ist der Drehpunkt nicht mehr bei [rot_pnt_long],
	sondern wird über die zwei Positionen der Drehgestelle/Achsen y1 und -y1.

	[boogies]
	y1

[boogies]
1.5

	////////////////////////////////////////////////////////
		Sinusoidal run and car body oscillations:
	////////////////////////////////////////////////////////

	The first command defines the sinusoidal run of the railroad vehicle:
	[sinus]
	{wheel radius}		
	{span between wheels, std.: 1.5m}
	{wheel tapering}
	{damping}

[sinus]
0.8
3
0.025
0.01

	The second entry defines the oscillating behaviour of the car body:

	[rail_body_osc]
	{vertical moment arm between boogie pins and center of gravity of body}
	{rotational oscilation around Y axle, angular frequency}
	{rotational oscilation around Y axle, damping}
	{rotational oscilation around X axle, angular frequency}
	{rotational oscilation around X axle, damping}
	{translational oscilation along Z axle, angular frequency}
	{translational oscilation along Z axle, damping}

[rail_body_osc]
0.9
6
6
25
17
8
4



	////////////////////////////////////////////////////////
		Cameras
	////////////////////////////////////////////////////////

	0: Blick nach vorne (std, Passagier)
[add_camera_pax]
0.05
0.1
0.5
-0.06
50
45
-22.5



[newachse]
achse_long
1.5
achse_maxwidth
1.606
achse_minwidth
1.284
achse_raddurchmesser
0.8
achse_feder
5000
achse_maxforce
1000
achse_daempfer
5000
achse_antrieb
0

[newachse]
achse_long
-1.5
achse_maxwidth
1.606
achse_minwidth
1.284
achse_raddurchmesser
0.8
achse_feder
5000
achse_maxforce
1000
achse_daempfer
5000
achse_antrieb
0
