[const]
engine_J
3.5

[const]
engine_e-gas
1

[const]
speedgov
59

[const]
rpmgov
3050

[const]
engine_power_idle
0

[const]
engine_Year
2017

[const]
eng_L
0

[const]
Max_Power
200


[newcurve]
engine_M_maxThrottle

[pnt]
0
1500

[pnt]
800
1500

[pnt]
3000
320

[pnt]
3050
0

[newcurve]
engine_M_minThrottle

[pnt]
1
1

[pnt]
2
0

[pnt]
3000
-10

[pnt]
3050
-30

[newcurve]
engine_efficiency_rpm

[pnt]
0
1

[pnt]
1000
1

[pnt]
3000
1

[pnt]
3050
0.1

[newcurve]
engine_efficiency_throttle

[pnt]
0
0

[pnt]
0.2
0.2

[pnt]
0.85
0.85

[pnt]
1
1

[newcurve]
engine_M_bremse

[pnt]
0
0

[pnt]
0.01
0.08

[pnt]
0.05
0.2

[pnt]
0.1
0.38

[pnt]
0.5
0.5

[pnt]
1
1

[newcurve]
engine_M_bremseF

[pnt]
3
0

[pnt]
5
0.6

[pnt]
35
0.75

[pnt]
45
1

[newcurve]
engine_braking

[pnt]
0
1

[pnt]
1
0

[const]
engine_consumption_curve_available
1

[newcurve]
engine_consumption_per_rpm

[pnt]
1
1040

[pnt]
3500
1040

[const]
luefterthermostat_opn
58

[const]
luefterthermostat_cls
55

[const]
kuehlerthermostat_opn
52

[const]
kuehlerthermostat_cls
50

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
95
0

[pnt]
100
100

[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
300

[const]
engine_Qrate_fan_factor
1.15

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000

First is turbocharger PSI
Second is the torque mutipler
[newcurve]
turbo_M_max

[pnt]
0
1

[pnt]
30
1

[pnt]
35
1.15

[newcurve]
turbo_limit_thorttle_1

[pnt]
0
5

[pnt]
0.85
30

[pnt]
1
35

Controls the turbo boost using the engine rpm 
[newcurve]
turbo_engine_rpm_efficiency

[pnt]
550
1.00

[pnt]
1000
1.1

[newcurve]
turbo_engine_rpm_max_psi
[pnt]
300
5

[pnt]
600
20

[pnt]
1200
30

[newcurve]
turbo_inertia

[pnt]
0
3

[pnt]
10
30

[pnt]
30
90

[newcurve]
turbo_inertia_dec

[pnt]
0
0.5


[pnt]
30
20

[newcurve]
turbo_M_inertia_throttle

[pnt]
0
0

[pnt]
1
0.85

[newcurve]
governor
[pnt]
-1
1

[pnt]
0.4
0.5

[pnt]
1
0

[pnt]
1.02
-0.001

[newcurve]
rpmgov_map

[pnt]
-75
1

[pnt]
0
0.1

[pnt]
2
0

[newcurve]
engine_airflow

[pnt]
0
1

[pnt]
10
2

[newcurve]
engine_efficiency_random

[pnt]
1
0.5

[pnt]
4
1

[pnt]
18
1

[pnt]
20
1.2
