[newcurve]
cockpit_tacholinie

[pnt]
0
0
[pnt]
5
2
[pnt]
10
7
[pnt]
20
20
[pnt]
30
31
[pnt]
40
63
[pnt]
50
84
[pnt]
60
106
[pnt]
70
127
[pnt]
80
150
[pnt]
90
171
[pnt]
100
193
[pnt]
110
215
[pnt]
120
234
[pnt]
125
245

[newcurve]
cockpit_oeldruck

[pnt]
300
0

[pnt]
400
1.1

[pnt]
1700
4.5


[newcurve]
cockpit_tensiune

[pnt]
0
1

[pnt]
300
1.5

[pnt]
400
1.75

[pnt]
500
2

[pnt
600
2

[pnt]
700
2

[pnt]
900
2.1

[pnt]
1100
2.2

[pnt]
1300
2.3

[pnt]
1500
2.4

[pnt]
1700
2.6

[pnt]
1900
2.7

[pnt]
2100
2.8

[pnt]
2300
2.8

[pnt]
2500
3

[pnt]
2800
4


[newcurve]
odometer_10er-uebertrag
[pnt]
0
0
[pnt]
0.9
0
[pnt]
1
1

[newcurve]
cockpit_engine_temperature

[pnt]
0
0

[pnt]
60
17

[pnt]
70
29

[pnt]
80
45

[pnt]
90
65

[pnt]
100
84

[pnt]
110
100


[const]
automatic_battery_switch
1

[const]
auxheat_via_button
0

[const]
wiper_lever
1

[newcurve]
cockpit_warndruck

[pnt]
550000
1

[pnt]
700000
0

[const]
cockpit_gangwahltaster_alt
0

[const]
cockpit_zentralschmierung_dist
50

[const]
cockpit_zentralschmierung_maxtime
30

[const]
cockpit_gear_D_only
1

[const]
cockpit_has_20h_switch
0

[const]
cockpit_has_door_0_lock_sw
1

[const]
cockpit_has_retarderswitch
1

[const]
cockpit_has_coolingswitch
0

[const]
cp_fahrertuer_anschlagseite
-1

[const]
cockpit_aftdoorlight_condition_D92
1

Blinking period (inverse frequency) for the Combined open door light - (1=static, 2= 0.5 Hz, etc.)
[const]
cockpit_tuerkontrolle_blinkperiod
2


=============================================
Inverse Widerstände (Leitwerte) in 1/Ohm.


Allgemeiner Stromverbrauch Panel (sonstige): 1x40W (1x0.0174 1/Ohm)

[const]
cp_general_Rinv
0.0174

[const]
cockpit_light_kneeling_selftesttime
2.0

[const]
cockpit_light_kneeling_failure_selftesttime
2.5

.............................

Frontheizgerät: 1x60W (1x0.104 1/Ohm)

[const]
cp_klimator_Rinv
0.104

.............................

Hintere Heizgeräte (zusammen): 60W (0.104 1/Ohm)

[const]
cp_cabinheater_Rinv
0.104
