
		Door Acceleration (100%/s�)

[const]
fdoor_acc
12.5

[const]
mdoor_acc
12.5

[const]
bdoor_acc
12.5

		Door Acceleration Variation (100%/s�)

[const]
door_acc_var
2.5

		Door Max Speed (100%/s)

[const]
fdoor_maxspeed
3

[const]
mdoor_maxspeed
3

[const]
bdoor_maxspeed
3

[const]
door_maxspeed_var
0.02

		Door Damper (100%/s)

[const]
door0_damper
22

[const]
door1_damper
22

[const]
door2_damper
22

[const]
door3_damper
22

[const]
door4_damper
22

[const]
door5_damper
22

		Damper characteristics

[newcurve]
damper_f_close

[pnt]
0.2
0.65

[pnt]
0.85
0.08

[newcurve]
damper_f_open

[pnt]
0
0

[pnt]
0.05
0

[pnt]
0.2
0.25

[pnt]
1
0.25

[newcurve]
damper_m_close

[pnt]
0.2
0.65

[pnt]
0.85
0.08

[newcurve]
damper_m_open

[pnt]
0
0

[pnt]
0.05
0

[pnt]
0.2
0.25

[pnt]
1
0.25

[newcurve]
damper_b_close

[pnt]
0.2
0.65

[pnt]
0.85
0.08

[newcurve]
damper_b_open

[pnt]
0
0

[pnt]
0.05
0

[pnt]
0.2
0.25

[pnt]
1
0.25

		Door Stop Reflexion Coefficient

[const]
door_refl
0.1

[const]
door_overlap_delay
1.4

		Automatic Back Door Time

[const]
doorMidOpenTime
0.9

[const]
doorAftOpenTime
0.9

		Busstop Brake will only be activated belov MaxKMH:

[const]
Door_Bremse_Halte_MaxKMH
2

'Front door wings are combined and rear doors is operated manually:

[const]
door_ManBackDoorFrontDoorCombined
1

'Safe-Reactivation:

[const]
door_safe_reactivating
1

[const]
door_stop_request_killed_by_front_door
1

[const]
door_stop_request_killed_by_back_door
1

Haltewunschlampe blink period (inverse frequency) - (1=static, 2= 0.5 Hz, etc.)
[const]
door_stop_request_blinkperiod
2

	Compressed-air doors

[const]
door_druckluft
1

[const]
door_needs_stopbrake
1

[const]
door_needs_stopbrakeswitch
1

[const]
electric_doors
0

[const]
thinking_doors
0

[const]
door_blocking
1

[const]
door_blocking_area
0.1

[const]
door_blocking_diff
0.01

[const]
door_blocking_speed
0.015

[newcurve]
door_0_opn_speed

[pnt]
0
1

[newcurve]
door_0_cls_speed

[pnt]
0
1

[newcurve]
door_1_opn_speed

[pnt]
0
1

[newcurve]
door_1_cls_speed

[pnt]
0
1


[newcurve]
door_2_opn_speed

[pnt]
0
1

[newcurve]
door_2_cls_speed

[pnt]
0
1

[newcurve]
door_3_opn_speed

[pnt]
0
1

[newcurve]
door_3_cls_speed

[pnt]
0
1

[newcurve]
door_4_opn_speed

[pnt]
0
1

[newcurve]
door_4_cls_speed

[pnt]
0
1

[newcurve]
door_5_opn_speed

[pnt]
0
1

[newcurve]
door_5_cls_speed

[pnt]
0
1


=============================================
Inverse Resistance (Conductance) in 1/Ohm.


Power Consumption: 150W/Speed 1 (0.260 1/Ohm)

[const]
door_Rinv
0.260

.............................
