	Front/Back Door Acceleration (100%/s²)

[const]
fdoor_acc
3

[const]
mdoor_acc
1.5

[const]
bdoor_acc
2.5

	Door Acceleration Variation (100%/s²)

[const]
door_acc_var
0.2

	Front/Back Door Max Speed (100%/s)

[const]
fdoor_maxspeed
1

[const]
mdoor_maxspeed
1.5

[const]
bdoor_maxspeed
1.5

[const]
door_maxspeed_var
0.02

	Front/Back Door Damper (100%/s)

[const]
door0_damper
12

[const]
door1_damper
2

[const]
door2_damper
12

[const]
door3_damper
2

[const]
door4_damper
12

[const]
door5_damper
2


		Dämpferkennlinie über Öffnungzustand:

[newcurve]
damper_f_close

[pnt]
0.2
1

[pnt]
0.8
0

[newcurve]
damper_f_open

[pnt]
0.2
0

[pnt]
0.8
0.8

[newcurve]
damper_m_close

[pnt]
0.2
1

[pnt]
0.8
0

[newcurve]
damper_m_open

[pnt]
0.2
0

[pnt]
0.8
0.6

[newcurve]
damper_b_close

[pnt]
0.2
1

[pnt]
0.8
0

[newcurve]
damper_b_open

[pnt]
0.2
0

[pnt]
0.8
0.6


	Door Stop Reflexion Coefficient

[const]
door_refl
0.2

	Automatic Back Door Time

[const]
doorMidOpenTime
4

[const]
doorAftOpenTime
4

  Haltewunsch von Automatiktür getrennt
  
[const]
door_RequestAndAutomaticSeparated
1

  Nur ein Haltewunsch-Kreis
  
[const]
door_OnlyOneRequest
1

	Busstop Brake will only be activated belov MaxKMH:

[const]
Door_Bremse_Halte_MaxKMH
2 

[const]
door_ManBackDoorFrontDoorCombined
2

0...Vordertürflügel einzeln, Mittel- und Hintertür automatisch
1...Vordertürflügel kombiniert, Mitteltür manuell und Hintertür automatisch
2...Vordertürflügel kombiniert, Mittel- und Hintertür automatisch

'Sicherheits-Rebelüftung:

[const]
door_safe_reactivating
1

[const]
door_stop_request_killed_by_front_door
1

[const]
door_druckluft
1

[const]
door_needs_stopbrake
0

[const]
door_needs_stopbrakeswitch
0

[const]
door_fixed_freigabe
0


[const]
electric_doors
0

[const]
thinking_doors
0

[const]
door_blocking
1

[const]
door_blocking_area
0.1

[const]
door_blocking_diff
0.03

[const]
door_blocking_speed
0.01





[newcurve]
door_0_opn_speed

[pnt]
0
1

[newcurve]
door_0_cls_speed

[pnt]
0
1

[newcurve]
door_1_opn_speed

[pnt]
0
1

[newcurve]
door_1_cls_speed

[pnt]
0
1

[newcurve]
door_2_opn_speed

[pnt]
0
1

[newcurve]
door_2_cls_speed

[pnt]
0
1

[newcurve]
door_3_opn_speed

[pnt]
0
1

[newcurve]
door_3_cls_speed

[pnt]
0
1

[newcurve]
door_4_opn_speed

[pnt]
0
1

[newcurve]
door_4_cls_speed

[pnt]
0
1

[newcurve]
door_5_opn_speed

[pnt]
0
1

[newcurve]
door_5_cls_speed

[pnt]
0
1


=============================================
Inverse Widerstände (Leitwerte) in 1/Ohm.


Türflügelstromverbrauch: 500W/Geschwindigkeit 1 (0.87 1/Ohm)

[const]
door_Rinv
0

.............................