[const]
Euro_4
0

[const]
Euro_6
1

[const]
Euro_6_cummins
0

[const]
engine_J
3.5

[newcurve]
max_rpm_idle

[pnt]
1490
1

[pnt]
1510
0

[newcurve]
hydroluefter_rpm

[pnt]
0
0

[pnt]
500
500

[pnt]
900
700

[pnt]
1300
1000

[pnt]
1900
1250

[const]
engine_speedcontrol
1

[newcurve]
max_speed

[pnt]
0
0.9

[pnt]
10
1.0

[pnt]
83
1

[pnt]
85
0.7

[pnt]
87
0
[const]
engine_e-gas
1

[const]
engine_ASR
1

[const]
engine_governed_idle_RPM
575

[const]
engine_governed_max_RPM
2200

[const]
engine_power_idle
22710

[const]
engine_coldM
-300

[newcurve]
engine_n_coldM

[pnt]
0
-140

[pnt]
2500
-350


[const]
engine_oelvis_M_nulldeg
-20

[const]
engine_oelvis_M_expfactor
-0.05

[const]
engine_RPM_ign_cold
150

[const]
engine_RPM_ign_warm
100

	Zeit [s], wie lange er "orgelt", wenn er gerade so die untere, "warme" Grenzdrehzahl erreicht:

[const]
engine_RPM_ign_time2warm
4


[const]
engine_starterM
1000

[const]
engine_starter_n_halbwert
67

[const]
engine_startering_sound_n_max
450

Mindeststrom, der immer durch den Starter fließt

[const]
engine_starter_minI
300

Ampere/Nm:

[const]
engine_starter_Ifaktor
0.5

[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
392
400

[pnt]
400
500

[pnt]
600
750

[pnt]
700
950

[pnt]
900
1300

[pnt]
1000
1400

[pnt]
1100
1400

[pnt]
1650
1400

[pnt]
1800
1225

[pnt]
1900
1100

[pnt]
2500
0


[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
300
400

[pnt]
575
0

[pnt]
650
-200

[pnt]
900
-500

[pnt]
2300
-600

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
0.6

[pnt]
1200
0.45

[pnt]
1700
0.45

[pnt]
2300
0.2

[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1.2

[const]
engine_fuel_value
16
9.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
240



[const]
luefterthermostat_opn
90

[const]
luefterthermostat_cls
87

[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
82

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
900

[const]
engine_Qrate_fan_factor
1.15

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000


[newcurve]
engine_turbo_RPM_factor

[pnt]
0
0

[pnt]
500
0.5

[pnt]
750
0.75

[pnt]
1000
1

[pnt]
1500
1

[pnt]
2000
1

[pnt]
2300
0.75


[newcurve]
engine_turbo_throttle_factor

[pnt]
0
0.5

[pnt]
1
1

[newcurve]
engine_turbo_boost

[pnt]
0
0.5

[pnt]
70
0.75

[pnt]
90
1

[pnt]
100
1