[const]
engine_J
3.5

[const]
engine_speedcontrol
0

[const]
engine_e-gas
0

[const]
engine_ASR
0

[const]
engine_governed_idle_RPM
575

[const]
engine_power_idle
22710

[const]
engine_coldM
-350

[newcurve]
engine_n_coldM

[pnt]
0
-140

[pnt]
2500
-350

[const]
engine_oelvis_M_nulldeg
-20

[const]
engine_oelvis_M_expfactor
-0.05

[const]
engine_RPM_ign_cold
150

[const]
engine_RPM_ign_warm
100

	Zeit [s], wie lange er "orgelt", wenn er gerade so die untere, "warme" Grenzdrehzahl erreicht:

[const]
engine_RPM_ign_time2warm
4


[const]
engine_starterM
1000

[const]
engine_starter_n_halbwert
67

[const]
engine_startering_sound_n_max
450

Mindeststrom, der immer durch den Starter fließt

[const]
engine_starter_minI
300

Ampere/Nm:

[const]
engine_starter_Ifaktor
0.5


[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
150
315

[pnt]
300
470

[pnt]
592
530

[pnt]
600
600

[pnt]
800
750

[pnt]
1000
800

[pnt]
1500
834

[pnt]
2000
800

[pnt]
2200
770

[pnt]
2250
0

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
150
300

[pnt]
450
300

[pnt]
631
0

[pnt]
750
-100

[pnt]
1000
-300

[pnt]
2500
-350

[newcurve]
engine_M_brake

[pnt]
50
0

[pnt]
300
-100

[pnt]
1000
-300

[pnt]
2000
-500

[const]
engine_brake_only_with_hard_gear
1



[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
0.6

[pnt]
1200
0.45

[pnt]
1700
0.45

[pnt]
2300
0.2

[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1.2

[const]
engine_fuel_value
16
9.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250


[const]
luefterthermostat_opn
90

[const]
luefterthermostat_cls
87

[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
82

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
300

[const]
engine_Qrate_fan_factor
1.15

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000



