[friendlyname]
S400 LE Business Series
S415LE FL - 1+2+0 - Ecolife
 White

[description]
The S400 LE Series is a well know group of intercity buses intended for short and medium distance travel.
These vehicles were produced between 2014 and 2023 in three lengths. They take the same base as its brother (O560) with a low entry floor in the front of the bus.
These vehicles have been a success all over the world in the Low Entry market. They are know for their versability and reliability aspect with their mixed use. They can be fitted to a "city" interior style to a "premium" interior maximizing passenger comfort and equipments. They are offered with options in terms of appearance, passenger equipment as well as engines and gearboxes.

- Technical Specifications -

Length: 12330 mm
Width: 2550 mm
Height: 3355 mm

Engine: OM 936, 7.7L, 220 kW, max. 1200 Nm
Gearbox: Automatic, 6-speed
Maximum speed: 100 km/h

Seating and standing places: 67 (42+25)
[end]

	[number] aktiviert die Zuweisung von Nummern
	{colorscheme specific numbers path}	Pfad zu den *.org-(Omsi-Registration)-Dateien, welche f�r die Vergabe von Nummern zust�ndig sind.

	Aufbau einer Nummernliste: in der ersten Zeile kommt der Name des Anstrichs (wie er auch im CTC angegeben wird), dann beliebig viele zul�ssige Nummern.
	Steht in der ersten Zeile nichts, dann handelt es sich um die "Hauptliste", welche f�r alle Anstriche gilt, f�r welche keine Nummern spezifiziert werden.


	[registration_automatic] aktiviert die Zuweisung der Kennzeichen im automatischen Modus
	{regPrefix}				Pr�fix vor Nummer am Kennzeichen. Soll bspw. Nr 2000 das Kennzeichen "D-A 2000H" bekommen, ist der Pr�fix "D-A "
	{regPostfix}				Postfix hinter Nummer am Kennzeichen. Im obigen Beispiel "H".

	[registration_list] �ffnet die angegebene Datei, um die Kennzeichenzuweisung nach den Nummern vorzunehmen. Der Index l�uft hierbei parallel zu jener *.org-Datei, welche die Hauptliste enth�lt.
	{filename}

	[registration_free] aktiviert die freie Kennzeichenzuweisung. Im AI-Modus wird ein Kennzeichen der Map-Registrations-Datei verwendet, der User kann es f�r sein Fahrzeug frei w�hlen.




[number]
Regs.org

	[registration_free]

[registration_automatic]
AA-GO 

[kmcounter_init]
2014
40000

[sound]
sound\sound_936_Mod.cfg

[sound_ai]
sound\sound_936_AI.cfg

[model]
model\S415LE_1-2-0.cfg

[paths]
model\paths_S415LE.cfg

[passengercabin]
model\passengercabin_S415LE.cfg

#########################
Scripts
#########################

[varnamelist]
19
script\S400_AI_varlist.txt
script\S400_Eco_varlist.txt
script\S400_Bremse_varlist.txt
script\S400_Cashdesk_varlist.txt
script\S400_Collision_varlist.txt
script\S400_Dashboard_varlist.txt
script\S400_Display_E6_varlist.txt
script\S400_Dirt_varlist.txt
script\S400_Elec_varlist.txt
script\S400_Heizung_varlist.txt
script\S400_IBIS_varlist.txt
script\S400_Engine_varlist.txt
script\S400_Klappern_varlist.txt
script\S400_Rain_varlist.txt
script\S400_Lights_varlist.txt
script\S400_Tuer_varlist.txt
script\S400_Wiper_varlist.txt
script\S400_VMatrix_varlist.txt
script\Urbino_II_Fare_varlist.txt

[stringvarnamelist]
5
script\S400_Dashboard_stringvarlist.txt
script\S400_Display_E6_stringvarlist.txt
script\S400_IBIS_stringvarlist.txt
script\S400_VMatrix_stringvarlist.txt
script\Urbino_II_Fare_stringvarlist.txt

[script]
21
script\S400_Main_Auto.osc
script\S400_Eco.osc
script\S400_Bremse.osc
script\S400_Cashdesk.osc
script\S400_Collision.osc
script\S400_Dashboard.osc
script\S400_Dirt.osc
script\S400_Display_E6.osc
script\S400_Elec.osc
script\S400_Engine.osc
script\S400_Forcefeedback.osc
script\S400_Heizung.osc
script\S400_IBIS.osc
script\S400_Klappern.osc
script\S400_Rain.osc
script\S400_Lights.osc
script\S400_Sound_volume.osc
script\S400_Tuer.osc
script\S400_Wiper.osc
script\S400_VMatrix.osc
script\Urbino_II_Fare.osc

[constfile]
18
script\S400_AI_constfile.txt
script\S400_Eco_6AP1400_constfile.txt
script\S400_Bremse_constfile.txt
script\S400_Collision_constfile.txt
script\S400_Dashboard_constfile.txt
script\S400_Dirt_constfile.txt
script\S400_Display_E6_constfile.txt
script\S400_Elec_constfile.txt
script\S400_Engine_constfile_936_220.txt
script\S400_Forcefeedback_constfile.txt
script\S400_Heizung_constfile.txt
script\S400_Klappern_constfile.txt
script\S400_Tuer_constfile_1-2-0.txt
script\S400_Tuer_constfileE6.txt
script\S400_Vmatrix_constfile.txt
script\S400_Lights_constfile.txt
script\S400_Wiper_constfile.txt
script\Urbino_II_fare_constfile.txt

#########################
Fahrersichten
#########################

[add_camera_driver]
-0.6878
5.660
2.100
-0.06
68
-110
0
[view_schedule]

[add_camera_driver]
-0.75
5.160
2.100
-0.06
68
-80
0

[add_camera_driver]
-0.6878
4.950
2.086
-0.06
60
-20
10

[add_camera_driver]
-0.6878
4.955
2.086
-0.06
62
0
-5

[add_camera_driver]
-0.6878
4.955
2.086
-0.06
60
35
5

[add_camera_driver]
-0.6878
5.155
2.123
-0.06
60
85
-8

[add_camera_driver]
-0.72
5.055
2.086
-0.06
45
40
-20
[view_ticketselling]



[add_camera_driver]
-0.72
5.355
2.123
-0.06
60
120
0


[add_camera_driver]
0
5.164
2.200
0
45
180
0

#########################
Passagiersichten
#########################

[add_camera_pax]
0
-5.259469
2.552
-0.06
45
0
0

[add_camera_pax]
0.905
-5.259469
2.552
-0.06
45
0
0



[add_camera_pax]
0.824044
4.428
2.23
0
55
-5
-5



[set_camera_std]
3

#########################

[set_camera_outside_center]
0
0
0.5

#########################
Reflexions kameras
#########################

[add_camera_reflexion_2]
-1.32
5.84
2.46
0
51
171
-17
1

[add_camera_reflexion]
1.49
6.73
2.47
0
50
208
-13
1

[add_camera_reflexion]
0.011
5.641
2.409
0
52
200
-20
0.15

[add_camera_reflexion]
0.378
-0.58
2.780
0
60
0
-17
0.15

[add_camera_reflexion]
0.71
6.82
2.50
0
110
65
40
0.15

#########################################
Physikalische und geometrische Grunddaten
#########################################

Masse in t:
[mass]
12

[momentofintertia]
360
100
360

Boundingbox des Busses *NEU01*

[boundingbox]
2.46
12.34
2.83
0
0.155
1.82

[schwerpunkt]
1.17

[rollwiderstand]
1000

[rot_pnt_long]
-2.705482

[inv_min_turnradius]
0.20

[ai_deltaheight]
-0.10

Front achse

[newachse]
achse_long
3.61911
achse_maxwidth
2.4
achse_minwidth
1.76
achse_raddurchmesser
1.035
achse_feder
214
achse_maxforce
71
achse_daempfer
20
achse_antrieb
0

Rear achse

[newachse]
achse_long
-2.705482
achse_maxwidth
2.4
achse_minwidth
1.2
achse_raddurchmesser
1.035
achse_feder
240
achse_maxforce
115
achse_daempfer
20
achse_antrieb
1