[friendlyname]
MAN
Lion's City A37 - Euro 6 - ZF - Ibox
White

[description]
This popular 2-door version of the Lion's City A37 bus with vertical engine arrangement is built by the German vehicle manufacturer, MAN. 

Specifications:-

Length: 11.9m
Width: 2.5m
Height: 2.88m

Engine: MAN D0836 (LOH66)
Power: 290 hp @ 2,200rpm

Gearbox: ZF 6-Speed
Maximum speed: 74 km/h

Empty weight: 11875 Kg
Gross weight: 18000 Kg

Seated: 37
Standing: 40
Wheelchair: 1
[end]

	[number] aktiviert die Zuweisung von Nummern
	{colorscheme specific numbers path}	Pfad zu den *.org-(Omsi-Registration)-Dateien, welche für die Vergabe von Nummern zuständig sind.

	Aufbau einer Nummernliste: in der ersten Zeile kommt der Name des Anstrichs (wie er auch im CTC angegeben wird), dann beliebig viele zulässige Nummern.
	Steht in der ersten Zeile nichts, dann handelt es sich um die "Hauptliste", welche für alle Anstriche gilt, für welche keine Nummern spezifiziert werden.


	[registration_automatic] aktiviert die Zuweisung der Kennzeichen im automatischen Modus
	{regPrefix}				Präfix vor Nummer am Kennzeichen. Soll bspw. Nr 2000 das Kennzeichen "D-A 2000H" bekommen, ist der Präfix "D-A "
	{regPostfix}				Postfix hinter Nummer am Kennzeichen. Im obigen Beispiel "H".

	[registration_list] öffnet die angegebene Datei, um die Kennzeichenzuweisung nach den Nummern vorzunehmen. Der Index läuft hierbei parallel zu jener *.org-Datei, welche die Hauptliste enthält.
	{filename}

	[registration_free] aktiviert die freie Kennzeichenzuweisung. Im AI-Modus wird ein Kennzeichen der Map-Registrations-Datei verwendet, der User kann es für sein Fahrzeug frei wählen.




[number]
Regs_A37.org

	[registration_free]

[registration_automatic]
M-AN 


[kmcounter_init]
2016
1000



[sound]
sound\d0836_zf-ecomat Ibox.cfg

[sound_ai]
sound\d0836_zf-ecomat Ibox.cfg

[model]
model\A37_Euro6 Ibox.cfg

[paths]
model\paths_A37.cfg

[passengercabin]
model\passengercabin_A37.cfg

	////////////////////////////////////////////////////////
		Scripts
	////////////////////////////////////////////////////////

[varnamelist]
23
script\AI_varlist.txt
script\Collision_varlist.txt
script\antrieb_ZF_varlist.txt
script\engine_varlist.txt
script\elec_varlist.txt
script\bremse_varlist.txt
script\auspuff_varlist.txt
script\lights_varlist.txt
script\door_varlist.txt
script\wiper_varlist.txt
script\cockpit_varlist.txt
script\klappern_varlist.txt
script\heizung_varlist.txt
script\rain_varlist.txt
script\dirt_varlist.txt
script\IBIS\ticketprinter_varlist.txt
script\churakrueger\VMatrix_varlist.txt
script\wimpel_varlist.txt
script\visual_varlist.txt
script\cashdesk_varlist.txt
script\MAN_dashboard_varlist.txt
script\spray_varlist.txt
script\IBIS\IBIS_varlist.txt

[stringvarnamelist]
5
script\IBIS\ticketprinter_stringvarlist.txt
script\churakrueger\vMatrix_stringvarlist.txt
script\cockpit_stringvarlist.txt
script\MAN_dashboard_stringvarlist.txt
script\IBIS\IBIS_stringvarlist.txt

[script]
27
script\AI.osc
script\main.osc
script\main_AI.osc
script\collision.osc
script\cockpit.osc
script\antrieb_ZF.osc
script\engine.osc
script\elec.osc
script\bremse.osc
script\auspuff.osc
script\lights.osc
script\door_auto.osc
script\wiper.osc
script\klappern.osc
script\forcefeedback.osc
script\rain.osc
script\dirt.osc
script\sound_volume.osc
script\heizung.osc
script\IBIS\Ticketprinter.osc
script\churakrueger\vmatrix.osc
script\wimpel.osc
script\cashdesk.osc
script\summer.osc
script\MAN_dashboard.osc
script\spray.osc
script\IBIS\IBIS-2.osc

[constfile]
18
script\AI_constfile.txt
script\collision_constfile.txt
script\antrieb_ZF_constfile.txt
script\engine_constfile_d0836_290hp.txt
script\elec_constfile.txt
script\bremse_constfile.txt
script\lights_constfile.txt
script\door_constfile.txt
script\auspuff_constfile.txt
script\cockpit_constfile.txt
script\klappern_constfile.txt
script\forcefeedback_constfile.txt
script\wiper_constfile.txt
script\dirt_constfile.txt
script\heizung_constfile.txt
script\IBIS\IBIS_constfile.txt
script\churakrueger\vmatrix_constfile_K++_pc.txt
script\MAN_dashboard_constfile.txt



	////////////////////////////////////////////////////////
		Kameras *NEU01*
	////////////////////////////////////////////////////////

	0: Looking leftmost
[add_camera_driver]
-1.5
4.18
1.89
-0.06
55
-170
-5
	1: Looking diagonally left
[add_camera_driver]
-0.70902
4.38
1.82
-0.06
55
-60
-5
	2: Looking into the left mirror
[add_camera_driver]
-0.70902
4.42
1.78
0
55
-30
-5

	3: Looking ahead (std)
[add_camera_driver]
-0.70902
4.42
1.78
0
50
0
-7

	4: Looking in the mirror right
[add_camera_driver]
-0.70902
4.42
1.78
0
55
35
-5

	5: At the door
[add_camera_driver]
-0.70902
4.38
1.82
-0.06
55
70
-6

	6: Ticket sales view
[add_camera_driver]
-0.73916
4.38
1.82
0
35
37
-16

[view_ticketselling]


	7: Looking far right
[add_camera_driver]
0
4.18
1.83
-0.06
55
160
-10


	8: Panel-Zoom
[add_camera_driver]
-0.73916
4.38
1.82
-0.06
55
5
-70

	7: Timetable view
[add_camera_driver]
-0.73916
4.38
1.82
-0.06
30
-30
45
[view_schedule]



################
Passagiersichten
################

	0: Hinten links sitzend
[add_camera_pax]
-0.943
-2.419
2
-0.06
45
25
0

	1: Stehplatz an der Hintertuer
[add_camera_pax]
-0.8
0.409
1.985
-0.06
45
90
0
	2: vorne rechts sitzend
[add_camera_pax]
0.967
1.374
1.554
-0.06
45
-20
0

	3: vorne rechts sitzend2
[add_camera_pax]
0.836
3.455
1.852
-0.06
45
-20
0

	2: hinten rechts sitzend
[add_camera_pax]
0.006
-5.516
2.1
-0.06
45
-20
0



	Folgender Befehl setzt die Standardfahrerkamera:

[set_camera_std]
3

	Folgender Befehl setzt den Zentrierpunkt der Au?enkamera:

[set_camera_outside_center]
0
0
1.2



	////////////////////////////////////////////////////////
		Reflexionskameras *NEU01*
	////////////////////////////////////////////////////////
	
[add_camera_reflexion_2]
-1.397
5.316
1.965
0
52
169
-10
0.15

[add_camera_reflexion]
1.358
6.214
2.033
0
52
201
-10

[add_camera_reflexion_2]
-0.005
5.2
2.576
0
52
195
-22
0.15


	////////////////////////////////////////////////////////
		Physikalische und geometrische Grunddaten
	////////////////////////////////////////////////////////

[mass]
11.9

[momentofintertia]
376.471500
90.5039999
376.471500

[boundingbox]
2.52
12
2.4
0
-0.35
1.7

[schwerpunkt]
1.1265

[rollwiderstand]
900

[rot_pnt_long]
-2.66472

[inv_min_turnradius]
0.16

[ai_deltaheight]
-0.10

	Front axle :

[newachse]
achse_long
3.18772
achse_maxwidth
2.339
achse_minwidth
1.765
achse_raddurchmesser
0.953
achse_feder
283.878000
achse_maxforce
72.45
achse_daempfer
20
achse_antrieb
0

	Rear axle:

[newachse]
achse_long
-2.66472
achse_maxwidth
2.36
achse_minwidth
1.086
achse_raddurchmesser
0.953
achse_feder
317.94336
achse_maxforce
115
achse_daempfer
20
achse_antrieb
1